type bt_firmware_file, file_type;
type rild, domain;

#me.phh.treble.qti.audio is system-signed
allow system_app hal_telephony_hwservice:hwservice_manager { find };
allow { rild system_app } { rild system_app }:binder { call transfer };

#Pixel 1
type vnd_qcril_audio_hwservice, hwservice_manager_type;
allow system_app vnd_qcril_audio_hwservice:hwservice_manager { find };

#Pixel 2
type vnd_qcrilhook_hwservice, hwservice_manager_type;
allow system_app vnd_qcrilhook_hwservice:hwservice_manager { find };

#OP6
allow system_app hal_telephony_hwservice:hwservice_manager { find };

# cf https://github.com/phhusson/treble_experimentations/issues/131
# SELinux : avc:  denied  { add } for interface=android.hardware.tetheroffload.control::IOffloadControl pid=15220 scontext=u:r:ipacm:s0 tcontext=u:object_r:hal_tetheroffload_hwservice:s0 tclass=hwservice_manager permissive=0
type ipacm, hwservice_manager_type;
allow ipacm hal_tetheroffload_hwservice:hwservice_manager { add };

type rpmb_device, file_type;
allow tee rpmb_device:blk_file rw_file_perms;
allowxperm tee rpmb_device:blk_file ioctl { 0xb300-0xbfff };

attribute smcinvoke_device_29_0;
type smcinvoke_device, dev_type;
typeattribute smcinvoke_device smcinvoke_device_29_0;
